		Headlight switch

	Off
	x
	x
	x
	x

	Low
	x
	
	
	

	High
	x
	
	
	

	Block this
	
	
	
	

	Tmnl
	5
	 (
Red
Black
6V Batt
Earth
)6
	7
	8


BSA A65 Lightning (Clubman?) Circuit diagram (12 Volt Negative earth) With Indicators
 (
Switch operation:
Off
Nothing on
Low
Side, rear  & speedo
/ tacho 
 lights
High
Headlight 
(main/ dip by handlebar sw
)
) (
Run 
Earths
 from :
Battery to frame
Battery to  engine
Battery to Headlamp 
Rear light
Wherever 
else 
suitable
)	


 (
Rd / Blk
12
 Volts 
Feed
Blu
Amm
Brn/ 
Grn
Blu      
Wht/ Vlt
Blu/ Brn
 ?
Dip switch (handlebars
)
Brn/ 
Grn
Red
Speedo 
light
Blu/ Wht 
Side light
Red
Brn
Earth
Red
Stop  light sw
Stop light
 
Blu
e 
Earth
Main Beam
White
Dipped  Beam
Tacho
 
light
red
Horn
Horn switch
Blk/ Grn
Rd / Blk
Red
Rear light
Eth- rear number plate
Rd / Blk
)	

		
				
 (
Fuse
Red
Red
Blk/ Wht
 
Blk/ Yell
 
Blk
Boyer Ign
 
Contact B
r
krs
White
Ign Sw
Blk/ Yell
Earth
Green
)		
				
								
 (
Yell
Red
Grn/ 
Blk
Earth
Reg/Rec
Bkk
Y
Y
R
Yell
Wh/ Grn
Alternator
)	
				

				
 (
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Earth
Earth
Light Blue
Left front
Right rear
Right front
Left rear
LED 
Flasher relay
Orange
Wht/ Vlt
Grey
Orange
Orange
Light Green
Pink
Dip Switch
Red
Pink
Red
Fuse
Indicator circuit
)				
	
	
